**SECTION 28 23 29**

**VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS**

**Advanced Technology Video CH7D37PB(S) Covert Height Strip Camera**

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

*This guide specification is intended for use by the design/construction professional and any user of Advanced Technology Video (ATV) products to assist in developing project specifications for security and video surveillance systems.*

*Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

1. **GENERAL**
   1. SUMMARY
      1. Section includes Video Surveillance Remote Devices and Sensors.
      2. Related Sections:
         1. Section 28 23 13 – Video Surveillance Control and Management Systems
         2. Section 28 23 16 – Video Surveillance Monitoring and Supervisory Interfaces
         3. Section 28 23 19 – Digital Video Recorders and Analog Recording Devices
         4. Section 28 23 23 – Video Surveillance Systems Infrastructure
   2. SYSTEM DESCRIPTION
      1. Description: Video surveillance and monitoring at points as indicated on Drawings.
         1. CH7D37PB(S): 700TVL, Day/Night, Covert Height Strip Camera
      2. Performance Requirements
         1. Color camera using a 1/3” CCD sensor
         2. Produces a minimum of 700TVL of horizontal resolution
         3. Day/Night functionality
         4. Covert camera housed in height strip metal enclosure with graduated and color coded height measurements in U.S. or Metric dimensions
         5. The camera shall be of manufacturer’s official product line, designed for commercial/industrial continuous 24/7 use.
         6. The camera shall be based upon standard components and proven technology.
   3. DEFINITIONS
      1. Covert Camera: a camera housed in a ordinary object one might find in a business or home that is capable of capturing video footage of activity that occurs within its’ view without the public’s knowledge
   4. SUBMITTALS
      1. Submit under provisions of Section 01 33 00 - Submittal procedures.
      2. Shop Drawings: Indicate electrical characteristics and connection requirements, including system wiring diagram.
      3. Product Data: Submit catalog data showing electrical characteristics and connection requirements for each component.
   5. CLOSEOUT SUBMITTALS
      1. Section 01 70 00 - Execution and Closeout Requirements: Closeout procedures.
      2. Project Record Documents: Record actual locations of cameras and routing of cabling.
      3. Operation and Maintenance Data: Submit instructions for operating system and performing routine trouble shooting procedures.
   6. QUALIFICATIONS
      1. Manufacturer: Company specializing in manufacturing products specified in this section with minimum ten years documented experience.
      2. Supplier: Authorized distributor of specified manufacturer with minimum 5 years documented experience.
      3. Installer: Authorized installer of specified manufacturer with 5 years documented experience and with service
   7. ENVIRONMENTAL REQUIREMENTS
      1. Section 01 60 00 - Product Requirements.
      2. Conform to manufacturer’s standard service conditions during and after installation of components.
   8. FIELD MEASUREMENTS
      1. Verify field measurements prior to fabrication.
   9. MAINTENANCE SERVICE
      1. Section 01 70 00 - Execution and Closeout Requirements: Maintenance service.
      2. Furnish service and maintenance of video surveillance system for one year from Date of Substantial Completion.
2. PRODUCTS
   1. CAMERAS
      1. Manufacturers:
         1. Advanced Technology Video
         2. Substitutions: Section 01 60 00 - Product Requirements: Not Permitted.
      2. Models: CH7D37PB (Black housing) and CH7D37PS (Silver housing)
      3. Product Description: 700TVL, Day/Night, Covert Height Strip Camera
      4. Camera Image Sensor: 1/3” CCD.
      5. Lens: 3.7mm pinhole, fixed iris
      6. General Requirements:
         1. Scene Illumination: 0.1Lux Color; 0.04Lux B/W
         2. Resolution: 700 TV lines, minimum
         3. Signal to noise: >50dB
         4. Synchronization: Internal
         5. Scanning System: 2:1 Interlace
         6. Video Output: 1.0Vp-p @ 75ohms
         7. Electronic (Digital) Day / Night
      7. Video Requirements and Adjustments (minimum):
         1. Pixels: 976(H) x 494(V)
         2. Scanning Frequency: 15.73KHz(H) x 59.94Hz(V)
         3. Electronic Shutter: 1/60sec ~ 1/100,000sec
         4. Day/Night: Auto
         5. White Balance: Auto(ATW)
         6. Auto Gain Control: On
         7. Side Light Compensation (SLC): Auto.
         8. Digital Noise Reduction: 2D-DNR
      8. Electrical:
         1. Input Power: 12 ~ 15VDC, +/- 10%: power supply included.
         2. Power Consumption:
            1. 130mA (1.5W)
      9. Mechanical:
         1. Pre-packaged, height strip metal housing in black or silver color to match standard commercial door frames
         2. Graduated and color coded height measurements in U.S. or Metric dimensions
         3. Swivel Bracket Allows Adjustment of the Camera’s View to Accommodate Double Doors
         4. Unique 5º Vertical Tilt lever on Back of Camera for Adjusting Vertical Camera Angle
         5. Position of Camera in Housing is Adjustable from the 5’-6” Level (default) to the 5’ Level
         6. Power Input: 2-Pin terminal block
         7. Video Output: BNC Connector
         8. Dimensions (WxHxD): 1.75” x 34.35” x 1.375” (44.45mm x 872.6mm x 34.9mm)
         9. Weight: 2.8lbs (1.26kg)
         10. Operating Temperature: 14ºF ~ 122ºF (-10ºC ~ +50ºC)
         11. Operating Humidity: 0 to 96% RH (non-condensing)
      10. Conformity Certifications:
          1. Federal Communications Commission (FCC)
          2. European Conformity (CE)
3. EXECUTION
   1. EXISTING WORK
      1. Disconnect and remove abandoned video surveillance equipment.
      2. Extend existing video surveillance installations using materials and methods compatible with existing installations as specified.
      3. Clean and repair existing video surveillance equipment remaining or to be reinstalled.
   2. EXAMINATION
      1. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation.
      2. Do not begin installation until unacceptable conditions are corrected.
   3. PREPARATION
      1. Protect devices from damage during construction.
   4. INSTALLATION
      1. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor drawings plans.
      2. Perform installation with qualified service personnel.
      3. Install devices in accordance with the National Electrical Code or applicable local codes.
      4. Ensure selected location is secure and offers protection from accidental damage.
         1. Ground and bond video surveillance equipment in accordance with Section 26 05 26.
      5. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference.
   5. FIELD QUALITY CONTROL
      1. Test snugness of mounting screws of all installed equipment.
      2. Test proper operation of all video system devices.
      3. Determine and report all problems to the manufacturer’s customer service department.
   6. MANUFACTURER'S FIELD SERVICES
      1. Section 01 40 00 - Quality Requirements: Manufacturer's field services.
      2. Furnish manufacturer’s field representative to supervise final wiring connections and system adjustments.
   7. ADJUSTING
      1. Section 01 70 00 - Execution and Closeout Requirements: Requirements for starting and adjusting.
      2. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions.
      3. Make any adjustment of camera settings to comply with specific customer’s need.
      4. Adjust manual lens irises to meet lighting conditions.
   8. DEMONSTRATION AND TRAINING
      1. Demonstrate at final inspection that video management system and devices function properly.
      2. Demonstrate at final inspection camera’s functionality and video recording capabilities.

END OF SECTION